# Emulation

QEMU’s Tiny Code Generator (TCG) provides the ability to emulate a number of CPU architectures on any supported host platform. Both System Emulation and User Mode Emulation are supported depending on the guest architecture.

Supported Guest Architectures for Emulation
Architecture (qemu name) | System | User | Notes
--- | --- | --- | ---
Alpha | Yes | Yes | Legacy 64 bit RISC ISA developed by DEC
Arm (arm, aarch64) | Yes | Yes | Wide range of features, see A-profile CPU architecture support for details
AVR | Yes | No | 8 bit micro controller, often used in maker projects
Hexagon | No | Yes | Family of DSPs by Qualcomm
PA-RISC (hppa) | Yes | Yes | A legacy RISC system used in HP’s old minicomputers
x86 (i386, x86_64) | Yes | Yes | The ubiquitous desktop PC CPU architecture, 32 and 64 bit.
LoongArch | Yes | Yes | A MIPS-like 64bit RISC architecture developed in China
m68k | Yes | Yes | Motorola 68000 variants and ColdFire
Microblaze | Yes | Yes | RISC based soft-core by Xilinx
MIPS (mips*) | Yes | Yes | Venerable RISC architecture originally out of Stanford University
OpenRISC | Yes | Yes | Open source RISC architecture developed by the OpenRISC community
Power (ppc, ppc64) | Yes | Yes | A general purpose RISC architecture now managed by IBM
RISC-V | Yes | Yes | An open standard RISC ISA maintained by RISC-V International
RX | Yes | No | A 32 bit micro controller developed by Renesas
s390x | Yes | Yes | A 64 bit CPU found in IBM’s System Z mainframes
sh4 | Yes | Yes | A 32 bit RISC embedded CPU developed by Hitachi
SPARC (sparc, sparc64) | Yes | Yes | A RISC ISA originally developed by Sun Microsystems
Tricore | Yes | No | A 32 bit RISC/uController/DSP developed by Infineon
Xtensa | Yes | Yes | A configurable 32 bit soft core now owned by Cadence

## Semihosting

Semihosting is a feature defined by the owner of the architecture to allow programs to interact with a debugging host system. On real hardware this is usually provided by an In-circuit emulator (ICE) hooked directly to the board. QEMU’s implementation allows for semihosting calls to be passed to the host system or via the `gdbstub`.

Generally semihosting makes it easier to bring up low level code before a more fully functional operating system has been enabled. On QEMU it also allows for embedded micro-controller code which typically doesn’t have a full libc to be run as “bare-metal” code under QEMU’s user-mode emulation. It is also useful for writing test cases and indeed a number of compiler suites as well as QEMU itself use semihosting calls to exit test code while reporting the success state.

Semihosting is only available using TCG emulation. This is because the instructions to trigger a semihosting call are typically reserved causing most hypervisors to trap and fault on them.

Warning

Semihosting inherently bypasses any isolation there may be between the guest and the host. As a result a program using semihosting can happily trash your host system. Some semihosting calls (e.g. `SYS_READC`) can block execution indefinitely. You should only ever run trusted code with semihosting enabled.

### Redirection

Semihosting calls can be re-directed to a (potentially remote) gdb during debugging via the gdbstub. Output to the semihosting console is configured as a `chardev` so can be redirected to a file, pipe or socket like any other `chardev` device.

### Supported Targets

Most targets offer similar semihosting implementations with some minor changes to define the appropriate instruction to encode the semihosting call and which registers hold the parameters. They tend to presents a simple POSIX-like API which allows your program to read and write files, access the console and some other basic interactions.

For full details of the ABI for a particular target, and the set of calls it provides, you should consult the semihosting specification for that architecture.

Note

QEMU makes an implementation decision to implement all file access in `O_BINARY` mode. The user-visible effect of this is regardless of the text/binary mode the program sets QEMU will always select a binary mode ensuring no line-terminator conversion is performed on input or output. This is because gdb semihosting support doesn’t make the distinction between the modes and magically processing line endings can be confusing.

Guest Architectures supporting Semihosting
Architecture | Modes | Specification
--- | --- | ---
Arm | System and User-mode | https://github.com/ARM-software/abi-aa/blob/main/semihosting/semihosting.rst
m68k | System | https://sourceware.org/git/?p=newlib-cygwin.git;a=blob;f=libgloss/m68k/m68k-semi.txt;hb=HEAD
MIPS | System | Unified Hosting Interface (MD01069)
RISC-V | System and User-mode | https://github.com/riscv/riscv-semihosting-spec/blob/main/riscv-semihosting-spec.adoc
Xtensa | System | Tensilica ISS SIMCALL

## TCG Plugins

QEMU TCG plugins provide a way for users to run experiments taking advantage of the total system control emulation can have over a guest. It provides a mechanism for plugins to subscribe to events during translation and execution and optionally callback into the plugin during these events. TCG plugins are unable to change the system state only monitor it passively. However they can do this down to an individual instruction granularity including potentially subscribing to all load and store operations.

See the developer section of the manual for details about writing plugins.

### Usage

Any QEMU binary with TCG support has plugins enabled by default. Earlier releases needed to be explicitly enabled with:

    configure --enable-plugins

Once built a program can be run with multiple plugins loaded each with their own arguments:

    $QEMU $OTHER_QEMU_ARGS \
        -plugin contrib/plugins/libhowvec.so,inline=on,count=hint \
        -plugin contrib/plugins/libhotblocks.so

Arguments are plugin specific and can be used to modify their behaviour. In this case the howvec plugin is being asked to use inline ops to count and break down the hint instructions by type.

Linux user-mode emulation also evaluates the environment variable `QEMU_PLUGIN`:

    QEMU_PLUGIN="file=contrib/plugins/libhowvec.so,inline=on,count=hint" $QEMU

QEMU plugins avoid to write directly to stdin/stderr, and use the log provided by the API (see function `qemu_plugin_outs`). To show output, you may use this additional parameter:

    $QEMU $OTHER_QEMU_ARGS \
      -d plugin \
      -plugin contrib/plugins/libhowvec.so,inline=on,count=hint

### Example Plugins

There are a number of plugins included with QEMU and you are encouraged to contribute your own plugins plugins upstream. There is a `contrib/plugins` directory where they can go. There are also some basic plugins that are used to test and exercise the API during the `make check-tcg` target in `tests/tcg/plugins` that are never the less useful for basic analysis.

#### Empty

`tests/tcg/plugins/empty.c`

Purely a test plugin for measuring the overhead of the plugins system itself. Does no instrumentation.

#### Basic Blocks

`tests/tcg/plugins/bb.c`

A very basic plugin which will measure execution in coarse terms as each basic block is executed. By default the results are shown once execution finishes:

    $ qemu-aarch64 -plugin tests/plugin/libbb.so \
        -d plugin ./tests/tcg/aarch64-linux-user/sha1
    SHA1=15dd99a1991e0b3826fede3deffc1feba42278e6
    bb's: 2277338, insns: 158483046

Behaviour can be tweaked with the following arguments:

Basic Block plugin arguments
Option | Description
--- | ---
inline=true|false | Use faster inline addition of a single counter.
idle=true|false | Dump the current execution stats whenever the guest vCPU idles

#### Basic Block Vectors

`contrib/plugins/bbv.c`

The bbv plugin allows you to generate basic block vectors for use with the SimPoint analysis tool.

Basic block vectors arguments
Option | Description
--- | ---
interval=N | The interval to generate a basic block vector specified by the number of instructions (Default: N = 100000000)
outfile=PATH | The path to output files. It will be suffixed with `.N.bb` where `N` is a vCPU index.

Example:

    $ qemu-aarch64 \
      -plugin contrib/plugins/libbbv.so,interval=100,outfile=sha1 \
      tests/tcg/aarch64-linux-user/sha1
    SHA1=15dd99a1991e0b3826fede3deffc1feba42278e6
    $ du sha1.0.bb
    23128   sha1.0.bb

#### Instruction

`tests/tcg/plugins/insn.c`

This is a basic instruction level instrumentation which can count the number of instructions executed on each core/thread:

    $ qemu-aarch64 -plugin tests/plugin/libinsn.so \
        -d plugin ./tests/tcg/aarch64-linux-user/threadcount
    Created 10 threads
    Done
    cpu 0 insns: 46765
    cpu 1 insns: 3694
    cpu 2 insns: 3694
    cpu 3 insns: 2994
    cpu 4 insns: 1497
    cpu 5 insns: 1497
    cpu 6 insns: 1497
    cpu 7 insns: 1497
    total insns: 63135

Behaviour can be tweaked with the following arguments:

Instruction plugin arguments
Option | Description
--- | ---
inline=true|false | Use faster inline addition of a single counter.
sizes=true|false | Give a summary of the instruction sizes for the execution
match=<string> | Only instrument instructions matching the string prefix

The `match` option will show some basic stats including how many instructions have executed since the last execution. For example:

    $ qemu-aarch64 -plugin tests/plugin/libinsn.so,match=bl \
        -d plugin ./tests/tcg/aarch64-linux-user/sha512-vector
    ...
    0x40069c, 'bl #0x4002b0', 10 hits, 1093 match hits, Δ+1257 since last match, 98 avg insns/match
    0x4006ac, 'bl #0x403690', 10 hits, 1094 match hits, Δ+47 since last match, 98 avg insns/match
    0x4037fc, 'bl #0x4002b0', 18 hits, 1095 match hits, Δ+22 since last match, 98 avg insns/match
    0x400720, 'bl #0x403690', 10 hits, 1096 match hits, Δ+58 since last match, 98 avg insns/match
    0x4037fc, 'bl #0x4002b0', 19 hits, 1097 match hits, Δ+22 since last match, 98 avg insns/match
    0x400730, 'bl #0x403690', 10 hits, 1098 match hits, Δ+33 since last match, 98 avg insns/match
    0x4037ac, 'bl #0x4002b0', 12 hits, 1099 match hits, Δ+20 since last match, 98 avg insns/match
    ...

For more detailed execution tracing see the `execlog` plugin for other options.

#### Memory

`tests/tcg/plugins/mem.c`

Basic instruction level memory instrumentation:

    $ qemu-aarch64 -plugin tests/plugin/libmem.so,inline=true \
        -d plugin ./tests/tcg/aarch64-linux-user/sha1
    SHA1=15dd99a1991e0b3826fede3deffc1feba42278e6
    inline mem accesses: 79525013

Behaviour can be tweaked with the following arguments:

Memory plugin arguments
Option | Description
--- | ---
inline=true|false | Use faster inline addition of a single counter
callback=true|false | Use callbacks on each memory instrumentation.
hwaddr=true|false | Count IO accesses (only for system emulation)

#### System Calls

`tests/tcg/plugins/syscall.c`

A basic syscall tracing plugin. This only works for user-mode. By default it will give a summary of syscall stats at the end of the run:

    $ qemu-aarch64 -plugin tests/plugin/libsyscall \
        -d plugin ./tests/tcg/aarch64-linux-user/threadcount
    Created 10 threads
    Done
    syscall no.  calls  errors
    226          12     0
    99           11     11
    115          11     0
    222          11     0
    93           10     0
    220          10     0
    233          10     0
    215          8      0
    214          4      0
    134          2      0
    64           2      0
    96           1      0
    94           1      0
    80           1      0
    261          1      0
    78           1      0
    160          1      0
    135          1      0

Behaviour can be tweaked with the following arguments:

Syscall plugin arguments
Option | Description
--- | ---
print=true|false | Print the number of times each syscall is called
log_writes=true|false | Log the buffer of each write syscall in hexdump format

#### Test inline operations

`tests/plugins/inline.c`

This plugin is used for testing all inline operations, conditional callbacks and scoreboard. It prints a per-cpu summary of all events.

#### Hot Blocks

`contrib/plugins/hotblocks.c`

The hotblocks plugin allows you to examine the where hot paths of execution are in your program. Once the program has finished you will get a sorted list of blocks reporting the starting PC, translation count, number of instructions and execution count. This will work best with linux-user execution as system emulation tends to generate re-translations as blocks from different programs get swapped in and out of system memory.

Example:

    $ qemu-aarch64 \
      -plugin contrib/plugins/libhotblocks.so -d plugin \
      ./tests/tcg/aarch64-linux-user/sha1
    SHA1=15dd99a1991e0b3826fede3deffc1feba42278e6
    collected 903 entries in the hash table
    pc, tcount, icount, ecount
    0x0000000041ed10, 1, 5, 66087
    0x000000004002b0, 1, 4, 66087
    ...

#### Hot Pages

`contrib/plugins/hotpages.c`

Similar to hotblocks but this time tracks memory accesses:

    $ qemu-aarch64 \
      -plugin contrib/plugins/libhotpages.so -d plugin \
      ./tests/tcg/aarch64-linux-user/sha1
    SHA1=15dd99a1991e0b3826fede3deffc1feba42278e6
    Addr, RCPUs, Reads, WCPUs, Writes
    0x000055007fe000, 0x0001, 31747952, 0x0001, 8835161
    0x000055007ff000, 0x0001, 29001054, 0x0001, 8780625
    0x00005500800000, 0x0001, 687465, 0x0001, 335857
    0x0000000048b000, 0x0001, 130594, 0x0001, 355
    0x0000000048a000, 0x0001, 1826, 0x0001, 11

The hotpages plugin can be configured using the following arguments:

Hot pages arguments
Option | Description
--- | ---
sortby=reads|writes|address | Log the data sorted by either the number of reads, the number of writes, or memory address. (Default: entries are sorted by the sum of reads and writes)
io=on | Track IO addresses. Only relevant to full system emulation. (Default: off)
pagesize=N | The page size used. (Default: N = 4096)

#### Instruction Distribution

`contrib/plugins/howvec.c`

This is an instruction classifier so can be used to count different types of instructions. It has a number of options to refine which get counted. You can give a value to the `count` argument for a class of instructions to break it down fully, so for example to see all the system registers accesses:

    $ qemu-system-aarch64 $(QEMU_ARGS) \
      -append "root=/dev/sda2 systemd.unit=benchmark.service" \
      -smp 4 -plugin ./contrib/plugins/libhowvec.so,count=sreg -d plugin

which will lead to a sorted list after the class breakdown:

    Instruction Classes:
    Class:   UDEF                   not counted
    Class:   SVE                    (68 hits)
    Class:   PCrel addr             (47789483 hits)
    Class:   Add/Sub (imm)          (192817388 hits)
    Class:   Logical (imm)          (93852565 hits)
    Class:   Move Wide (imm)        (76398116 hits)
    Class:   Bitfield               (44706084 hits)
    Class:   Extract                (5499257 hits)
    Class:   Cond Branch (imm)      (147202932 hits)
    Class:   Exception Gen          (193581 hits)
    Class:     NOP                  not counted
    Class:   Hints                  (6652291 hits)
    Class:   Barriers               (8001661 hits)
    Class:   PSTATE                 (1801695 hits)
    Class:   System Insn            (6385349 hits)
    Class:   System Reg             counted individually
    Class:   Branch (reg)           (69497127 hits)
    Class:   Branch (imm)           (84393665 hits)
    Class:   Cmp & Branch           (110929659 hits)
    Class:   Tst & Branch           (44681442 hits)
    Class:   AdvSimd ldstmult       (736 hits)
    Class:   ldst excl              (9098783 hits)
    Class:   Load Reg (lit)         (87189424 hits)
    Class:   ldst noalloc pair      (3264433 hits)
    Class:   ldst pair              (412526434 hits)
    Class:   ldst reg (imm)         (314734576 hits)
    Class: Loads & Stores           (2117774 hits)
    Class: Data Proc Reg            (223519077 hits)
    Class: Scalar FP                (31657954 hits)
    Individual Instructions:
    Instr: mrs x0, sp_el0           (2682661 hits)  (op=0xd5384100/  System Reg)
    Instr: mrs x1, tpidr_el2        (1789339 hits)  (op=0xd53cd041/  System Reg)
    Instr: mrs x2, tpidr_el2        (1513494 hits)  (op=0xd53cd042/  System Reg)
    Instr: mrs x0, tpidr_el2        (1490823 hits)  (op=0xd53cd040/  System Reg)
    Instr: mrs x1, sp_el0           (933793 hits)   (op=0xd5384101/  System Reg)
    Instr: mrs x2, sp_el0           (699516 hits)   (op=0xd5384102/  System Reg)
    Instr: mrs x4, tpidr_el2        (528437 hits)   (op=0xd53cd044/  System Reg)
    Instr: mrs x30, ttbr1_el1       (480776 hits)   (op=0xd538203e/  System Reg)
    Instr: msr ttbr1_el1, x30       (480713 hits)   (op=0xd518203e/  System Reg)
    Instr: msr vbar_el1, x30        (480671 hits)   (op=0xd518c01e/  System Reg)
    ...

To find the argument shorthand for the class you need to examine the source code of the plugin at the moment, specifically the `*opt` argument in the InsnClassExecCount tables.

#### Lockstep Execution

`contrib/plugins/lockstep.c`

This is a debugging tool for developers who want to find out when and where execution diverges after a subtle change to TCG code generation. It is not an exact science and results are likely to be mixed once asynchronous events are introduced. While the use of -icount can introduce determinism to the execution flow it doesn’t always follow the translation sequence will be exactly the same. Typically this is caused by a timer firing to service the GUI causing a block to end early. However in some cases it has proved to be useful in pointing people at roughly where execution diverges. The only argument you need for the plugin is a path for the socket the two instances will communicate over:

    $ qemu-system-sparc -monitor none -parallel none \
      -net none -M SS-20 -m 256 -kernel day11/zImage.elf \
      -plugin ./contrib/plugins/liblockstep.so,sockpath=lockstep-sparc.sock \
      -d plugin,nochain

which will eventually report:

    qemu-system-sparc: warning: nic lance.0 has no peer
    @ 0x000000ffd06678 vs 0x000000ffd001e0 (2/1 since last)
    @ 0x000000ffd07d9c vs 0x000000ffd06678 (3/1 since last)
    Δ insn_count @ 0x000000ffd07d9c (809900609) vs 0x000000ffd06678 (809900612)
      previously @ 0x000000ffd06678/10 (809900609 insns)
      previously @ 0x000000ffd001e0/4 (809900599 insns)
      previously @ 0x000000ffd080ac/2 (809900595 insns)
      previously @ 0x000000ffd08098/5 (809900593 insns)
      previously @ 0x000000ffd080c0/1 (809900588 insns)

#### Hardware Profile

`contrib/plugins/hwprofile.c`

The hwprofile tool can only be used with system emulation and allows the user to see what hardware is accessed how often. It has a number of options:

Hardware Profile arguments
Option | Description
--- | ---
track=[read|write] | By default the plugin tracks both reads and writes. You can use this option to limit the tracking to just one class of accesses.
source | Will include a detailed break down of what the guest PC that made the access was. Not compatible with the pattern option. Example output:
    cirrus-low-memory @ 0xfffffd00000a0000
     pc:fffffc0000005cdc, 1, 256
     pc:fffffc0000005ce8, 1, 256
     pc:fffffc0000005cec, 1, 256
pattern | Instead break down the accesses based on the offset into the HW region. This can be useful for seeing the most used registers of a device. Example output:
    pci0-conf @ 0xfffffd01fe000000
      off:00000004, 1, 1
      off:00000010, 1, 3
      off:00000014, 1, 3
      off:00000018, 1, 2
      off:0000001c, 1, 2
      off:00000020, 1, 2
      ...

#### Execution Log

`contrib/plugins/execlog.c`

The execlog tool traces executed instructions with memory access. It can be used for debugging and security analysis purposes. Please be aware that this will generate a lot of output.

The plugin needs default argument:

    $ qemu-system-arm $(QEMU_ARGS) \
      -plugin ./contrib/plugins/libexeclog.so -d plugin

which will output an execution trace following this structure:

    # vCPU, vAddr, opcode, disassembly[, load/store, memory addr, device]...
    0, 0xa12, 0xf8012400, "movs r4, #0"
    0, 0xa14, 0xf87f42b4, "cmp r4, r6"
    0, 0xa16, 0xd206, "bhs #0xa26"
    0, 0xa18, 0xfff94803, "ldr r0, [pc, #0xc]", load, 0x00010a28, RAM
    0, 0xa1a, 0xf989f000, "bl #0xd30"
    0, 0xd30, 0xfff9b510, "push {r4, lr}", store, 0x20003ee0, RAM, store, 0x20003ee4, RAM
    0, 0xd32, 0xf9893014, "adds r0, #0x14"
    0, 0xd34, 0xf9c8f000, "bl #0x10c8"
    0, 0x10c8, 0xfff96c43, "ldr r3, [r0, #0x44]", load, 0x200000e4, RAM

Please note that you need to configure QEMU with Capstone support to get disassembly.

The output can be filtered to only track certain instructions or addresses using the `ifilter` or `afilter` options. You can stack the arguments if required:

    $ qemu-system-arm $(QEMU_ARGS) \
      -plugin ./contrib/plugins/libexeclog.so,ifilter=st1w,afilter=0x40001808 -d plugin

This plugin can also dump registers when they change value. Specify the name of the registers with multiple `reg` options. You can also use glob style matching if you wish:

    $ qemu-system-arm $(QEMU_ARGS) \
      -plugin ./contrib/plugins/libexeclog.so,reg=\*_el2,reg=sp -d plugin

Be aware that each additional register to check will slow down execution quite considerably. You can optimise the number of register checks done by using the rdisas option. This will only instrument instructions that mention the registers in question in disassembly. This is not foolproof as some instructions implicitly change instructions. You can use the ifilter to catch these cases:

    $ qemu-system-arm $(QEMU_ARGS) \
      -plugin ./contrib/plugins/libexeclog.so,ifilter=msr,ifilter=blr,reg=x30,reg=\*_el1,rdisas=on

#### Cache Modelling

`contrib/plugins/cache.c`

Cache modelling plugin that measures the performance of a given L1 cache configuration, and optionally a unified L2 per-core cache when a given working set is run:

    $ qemu-x86_64 -plugin ./contrib/plugins/libcache.so \
        -d plugin -D cache.log ./tests/tcg/x86_64-linux-user/float_convs

will report the following:

    core #, data accesses, data misses, dmiss rate, insn accesses, insn misses, imiss rate
    0       996695         508             0.0510%  2642799        18617           0.7044%

    address, data misses, instruction
    0x424f1e (_int_malloc), 109, movq %rax, 8(%rcx)
    0x41f395 (_IO_default_xsputn), 49, movb %dl, (%rdi, %rax)
    0x42584d (ptmalloc_init.part.0), 33, movaps %xmm0, (%rax)
    0x454d48 (__tunables_init), 20, cmpb $0, (%r8)
    ...

    address, fetch misses, instruction
    0x4160a0 (__vfprintf_internal), 744, movl $1, %ebx
    0x41f0a0 (_IO_setb), 744, endbr64
    0x415882 (__vfprintf_internal), 744, movq %r12, %rdi
    0x4268a0 (__malloc), 696, andq $0xfffffffffffffff0, %rax
    ...

The plugin has a number of arguments, all of them are optional:

Cache modelling arguments
Option | Description
--- | ---
limit=N | Print top N icache and dcache thrashing instructions along with their address, number of misses, and its disassembly. (default: 32)
icachesize=N iblksize=B iassoc=A | Instruction cache configuration arguments. They specify the cache size, block size, and associativity of the instruction cache, respectively. (default: N = 16384, B = 64, A = 8)
dcachesize=N | Data cache size (default: 16834)
dblksize=B | Data cache block size (default: 64)
dassoc=A | Data cache associativity (default: 8)
evict=POLICY | Sets the eviction policy to POLICY. Available policies are: `lru`, `fifo`, and `rand`. The plugin will use the specified policy for both instruction and data caches. (default: POLICY = `lru`)
cores=N | Sets the number of cores for which we maintain separate icache and dcache. (default: for linux-user, N = 1, for full system emulation: N = cores available to guest)
l2=on | Simulates a unified L2 cache (stores blocks for both instructions and data) using the default L2 configuration (cache size = 2MB, associativity = 16-way, block size = 64B).
l2cachesize=N | L2 cache size (default: 2097152 (2MB)), implies `l2=on`
l2blksize=B | L2 cache block size (default: 64), implies `l2=on`
l2assoc=A | L2 cache associativity (default: 16), implies `l2=on`

#### Stop on Trigger

`contrib/plugins/stoptrigger.c`

The stoptrigger plugin allows to setup triggers to stop emulation. It can be used for research purposes to launch some code and precisely stop it and understand where its execution flow went.

Two types of triggers can be configured: a count of instructions to stop at, or an address to stop at. Multiple triggers can be set at once.

By default, QEMU will exit with return code 0. A custom return code can be configured for each trigger using `:CODE` syntax.

For example, to stop at the 20-th instruction with return code 41, at address 0xd4 with return code 0 or at address 0xd8 with return code 42:

    $ qemu-system-aarch64 $(QEMU_ARGS) \
      -plugin ./contrib/plugins/libstoptrigger.so,icount=20:41,addr=0xd4,addr=0xd8:42 -d plugin

The plugin will log the reason of exit, for example:

    0xd4 reached, exiting

#### Limit instructions per second

This plugin can limit the number of Instructions Per Second that are executed:

    # get number of instructions
    $ num_insn=$(./build/qemu-x86_64 -plugin ./build/tests/plugin/libinsn.so -d plugin /bin/true |& grep total | sed -e 's/.*: //')
    # limit speed to execute in 10 seconds
    $ time ./build/qemu-x86_64 -plugin ./build/contrib/plugins/libips.so,ips=$(($num_insn/10)) /bin/true
    real 10.000s

IPS arguments
Option | Description
--- | ---
ips=N | Maximum number of instructions per cpu that can be executed in one second. The plugin will sleep when the given number of instructions is reached.

## Other emulation features

When running system emulation you can also enable deterministic execution which allows for repeatable record/replay debugging. See Record/Replay for more details.