# virtio pmem

This document explains the setup and usage of the virtio pmem device. The virtio pmem device is a paravirtualized persistent memory device on regular (i.e non-NVDIMM) storage.

## Usecase

Virtio pmem allows to bypass the guest page cache and directly use host page cache. This reduces guest memory footprint as the host can make efficient memory reclaim decisions under memory pressure.

## How does virtio-pmem compare to the nvdimm emulation?

NVDIMM emulation on regular (i.e. non-NVDIMM) host storage does not persist the guest writes as there are no defined semantics in the device specification. The virtio pmem device provides guest write persistence on non-NVDIMM host storage.

## virtio pmem usage

A virtio pmem device backed by a memory-backend-file can be created on the QEMU command line as in the following example:

    -object memory-backend-file,id=mem1,share,mem-path=./virtio_pmem.img,size=4G
    -device virtio-pmem-pci,memdev=mem1,id=nv1

where:

> - “object memory-backend-file,id=mem1,share,mem-path=<image>, size=<image size>” creates a backend file with the specified size.

> - “device virtio-pmem-pci,id=nvdimm1,memdev=mem1” creates a virtio pmem pci device whose storage is provided by above memory backend device.

Multiple virtio pmem devices can be created if multiple pairs of “-object” and “-device” are provided.

## Hotplug

Virtio pmem devices can be hotplugged via the QEMU monitor. First, the memory backing has to be added via ‘object_add’; afterwards, the virtio pmem device can be added via ‘device_add’.

For example, the following commands add another 4GB virtio pmem device to the guest:

    (qemu) object_add memory-backend-file,id=mem2,share=on,mem-path=virtio_pmem2.img,size=4G
    (qemu) device_add virtio-pmem-pci,id=virtio_pmem2,memdev=mem2

## Guest Data Persistence

Guest data persistence on non-NVDIMM requires guest userspace applications to perform fsync/msync. This is different from a real nvdimm backend where no additional fsync/msync is required. This is to persist guest writes in host backing file which otherwise remains in host page cache and there is risk of losing the data in case of power failure.

With virtio pmem device, MAP_SYNC mmap flag is not supported. This provides a hint to application to perform fsync for write persistence.

## Limitations

- Real nvdimm device backend is not supported.

- virtio pmem hotunplug is not supported.

- ACPI NVDIMM features like regions/namespaces are not supported.

- ndctl command is not supported.